Lab 3, Part B:

B1. 0x1d1c1b1a

B2. 0x10010001

B3. 0x1a1b1c1d

B4. 0x1a

B5. 0x1d

B6. The MIPS Simulator is in **little endian**, because the least significant byte is first.